####################################################
#  SilverSat SSDV Image Creator(SSIC) ver.1.0
#  Windows Console Program written in Python3
#  Released on January 25, 2026
#  (c) 2026- JA3TDW/Fumio Asai All Rights Reserved
####################################################

1.SilverSat SSDV Image Creator(SSIC)とは
　SSICはオーブン衛星データーベースSatNOGS DBに蓄積された
SilverSatのSSDVフレームデータから撮影画像を生成するための
ソフトです。Python3のスクリプトをNuitkaで実行プログラム
(ssci.exe)を作成しています。

2.動作環境
)Winmdows 11 Home 64bit日本語版で動作を確認しています。
  Python3の実行環境は必要ありません。
2)SSICはSSDV画像データのエンコード/デコード用ソフトを
  呼び出して画像を生成するので、以下のWebサイトのソース
  ファイルから実行プログラム(ssdv.exe)を作成し、SSICと
  同じフォルダに入れて下さい。
* https://github.com/fsphil/ssdv
　
3.使用方法
1)SatNOGSからSilverSatのcsvファイルをダウンロードします。
2)ssic.exeを実行してcsvファイル名と画像IDを入力すると、
　SSDVフレームデータのcsvファイル(xx_output.csv)とbin
　ファイル(xx_output.bin)、画像ファイル(xx_output.jpg)
　がそれぞれ生成されます。xxは画像IDです。
*抽出されたSSDVフレームデータは重複が解消され、パケット
　ID順にソートされてcsvファイルに保存されます。
*binファイルはssdv.exe用のバイナリファイルです。

----------- SSICの実行画面例 ----------------
SilverSat SSDV Image Creator(SSIC) ver.1.0

Input csv file:input.csv
Press Enter key if csv file name is OK
Enter input csv file name:satnogs_input.csv
Enter image ID:18

Created SSDV frame file :18_output.csv
Created SSDV binary file:18_output.bin

Creating SSDV Image using ssdv.exe...
Callsign: WP2XGW
Image ID: 18
Resolution: 320x240
MCU blocks: 300
Sampling factor: 2x2
Quality level: 4
Read 65 packets
done
SSCI is going to close in 10 seconds...
-------------------------------------------

*リリースノート
1)2026/ 01/26:ver.1.0を公開
